Available Internet Bandwidth: 1000 Mbps

Internet Port (1:1) pure up to 1000 Mbps as follows:

1000 Mbps on fiber

1000 Mbps on standby fiber link in case one fiber link fails. Both fiber links are independent throughout the span from the service provider to AKGEC server room.

In addition, 200 Mbps is available on radio link, as standby in case of failure and unavailability of both fiber link

|  |  |  |
| --- | --- | --- |
| **Year** | **Bandwidth of Internet connection** | **Bill attached (yes/no)** |
| 2020-2021 | 1000 Mbps on fiber and 100 Mbps on Radio link | Yes |